Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro

Supermicro X7DBE (Intel Xeon 5160)

SPECint^®_rate2006 = Not Run

SPECint_rate_base2006 = 45.2

CPU2006 license: 49 Test date: Apr-2006 Test sponsor: Advanced Micro Devices Hardware Availability: Jul-2006 Tested by: Advanced Micro Devices Software Availability: Jul-2006

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate_base2006 = 45.2

0 99.0

6.00 12.0 18.0 24.0 30.0 36.0 42.0 48.0 54.0 60.0 66.0 72.0 78.0 84.0 90.0 4 76.7 4 46.5 4 43.2 4 29.1 4 64.2 4 47.1 4 71.0 4 30.6 4 98.9 4 26.8 4 35.8 4 26.2

Hardware

CPU Name: Intel Xeon 5160 CPU Characteristics: 3.0GHz 1333MHz System Bus CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 1,2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 8 GB (8 x 1 GB DDR2-667 CL5 ECC FB) Disk Subsystem: 250GB SATA Other Hardware: None

Software

Operating System: SUSE Linux 10.1 (for x86_64) Compiler: SUSE gcc, g++ 4.1 (for x86_64) Auto Parallel: No File System: ext3 System State: runlevel 3 Base Pointers: 64-bit Peak Pointers: Not Applicable Other Software: None

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro

Supermicro X7DBE (Intel Xeon 5160)

SPECint_rate2006 = Not Run SPECint_rate_base2006 = 45.2

CPU2006 license: 49 Test date: Apr-2006 Test sponsor: Advanced Micro Devices Hardware Availability: Jul-2006 Tested by: Advanced Micro Devices Software Availability: Jul-2006

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 4 508 77.0 513 76.2 510 76.7 401.bzip2 4 818 47.2 834 46.3 830 46.5 403.gcc 4 741 43.5 749 43.0 745 43.2 429.mcf 4 1255 29.1 1255 29.1 1256 29.0 445.gobmk 4 655 64.1 653 64.2 654 64.2 456.hmmer 4 793 47.1 792 47.1 794 47.0 458.sjeng 4 682 71.0 681 71.1 683 70.9 462.libquantum 4 2709 30.6 2711 30.6 2711 30.6 464.h264ref 4 897 98.7 895 98.9 895 98.9 471.omnetpp 4 931 26.9 933 26.8 933 26.8 473.astar 4 783 35.8 784 35.8 784 35.8 483.xalancbmk 4 1052 26.2 1052 26.2 1053 26.2

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

General Notes

 The system can be assembled using an SSI EEB form-factor case,
 and a Zippy/Emacs 700 watt PSL-6701P Power Supply.
Other Configuration Notes
 Taskset utility used to bind process to cores

Base Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Base Portability Flags

400.perlbench: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX_X64 401.bzip2: -DSPEC_CPU_LP64

403.gcc: -DSPEC_CPU_LP64 429.mcf: -DSPEC_CPU_LP64 445.gobmk: -DSPEC_CPU_LP64 456.hmmer: -DSPEC_CPU_LP64

458.sjeng: -DSPEC_CPU_LP64 462.libquantum: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro

Supermicro X7DBE (Intel Xeon 5160)

SPECint_rate2006 = Not Run SPECint_rate_base2006 = 45.2

CPU2006 license: 49 Test date: Apr-2006 Test sponsor: Advanced Micro Devices Hardware Availability: Jul-2006 Tested by: Advanced Micro Devices Software Availability: Jul-2006

Base Portability Flags (Continued)

464.h264ref: -DSPEC_CPU_LP64 471.omnetpp: -DSPEC_CPU_LP64

473.astar: -DSPEC_CPU_LP64 483.xalancbmk: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX

Base Optimization Flags

C benchmarks:

-O3 -fno-inline-functions -funroll-loops

C++ benchmarks:

-O3 -funroll-loops

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090714.04.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090714.04.xml

Originally published on 3 October 2006.

Report generated on Tue Jul 22 10:08:22 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance