Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M8000

SPECint^®_rate2006 = 335

SPECint_rate_base2006 = 285

CPU2006 license: 6 Test date: Mar-2007 Test sponsor: Sun Microsystems Hardware Availability: Apr-2007 Tested by: Sun Microsystems Software Availability: Jul-2007

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 335

SPECint_rate_base2006 = 285

0 650

30.0 60.0 90.0 120 140 160 180 200 220 240 260 280 300 320 340 360 380 400 420 440 460 480 500 520 540 560 580 600 620 63 320 32 426

63 224 32 307

63 246 63 257

63 366 63 373

63 319 32 374

63 258 32 269

63 254 63 279

63 635 63 643

63 426 32 614

63 131 63 166

63 205 63 242

63 291 63 357

Hardware

CPU Name: SPARC64 VI CPU Characteristics: CPU MHz: 2280 FPU: Integrated CPU(s) enabled: 32 cores, 16 chips, 2 cores/chip, 2 threads/core CPU(s) orderable: 1 to 4 CMUs; each CMU contains 2 or 4 chips Primary Cache: 128 KB I + 128 KB D on chip per core Secondary Cache: 5 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 256 GB (128 x 2 GB) Disk Subsystem: 400 GB Solaris Volume Manager RAID0 soft partition (see notes for details) Other Hardware: None

Software

Operating System: Solaris 10 7/07 (build s10s_u4wos_03) Compiler: Sun Studio 12 (build 44.0) Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: None

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M8000

SPECint_rate2006 = 335

SPECint_rate_base2006 = 285

CPU2006 license: 6 Test date: Mar-2007 Test sponsor: Sun Microsystems Hardware Availability: Apr-2007 Tested by: Sun Microsystems Software Availability: Jul-2007

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 63 1945 316 1924 320 1924 320 32 735 426 733 426 733 426

401.bzip2 63 2762 220 2718 224 2717 224 32 1005 307 1011 305 1004 307

403.gcc 63 2059 246 2065 246 2066 246 63 1977 257 1973 257 1971 257

429.mcf 63 1571 366 1569 366 1570 366 63 1539 373 1542 373 1537 374

445.gobmk 63 2078 318 2069 319 2065 320 32 897 374 898 374 899 373

456.hmmer 63 2277 258 2276 258 2275 258 32 1110 269 1110 269 1110 269

458.sjeng 63 3001 254 3004 254 2999 254 63 2736 279 2737 279 2737 279

462.libquantum 63 2055 635 2057 635 2056 635 63 2030 643 2030 643 2031 643

464.h264ref 63 3281 425 3274 426 3269 427 32 1152 615 1154 614 1153 614

471.omnetpp 63 3018 130 3017 131 3017 131 63 2382 165 2367 166 2371 166

473.astar 63 2160 205 2160 205 2155 205 63 1827 242 1825 242 1826 242

483.xalancbmk 63 1506 289 1494 291 1493 291 63 1218 357 1219 357 1226 355

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

Processes were bound to cores using "submit" and "pbind".
The SPEC toolset was bound to processor 0.

These shell commands request use of local 4MB pages:
      export LD_PRELOAD=madv.so.1:mpss.so.1
      export MPSSHEAP=4MB
      export MPSSSTACK=4MB
      export MADV=access_lwp
’access_lwp’ means that the next light weight
process to touch the specified address range
will access it the most heavily.

ulimit -s 131072 was used to limit the space
consumed by the stack (and therefore make more
space available to the heap).

 /etc/system parameters
    autoup=300
       Causes pages older than the listed number of seconds to
       be written by fsflush.
    bufhwm=3000
       Memory byte limit for caching I/O buffers
    segmap_percent=1
       Set maximum percent memory for file system cache
    tune_t_fsflushr=3
       Controls how many seconds elapse between runs of the
       page flush daemon, fsflush._{Continued on next page}

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M8000

SPECint_rate2006 = 335

SPECint_rate_base2006 = 285

CPU2006 license: 6 Test date: Mar-2007 Test sponsor: Sun Microsystems Hardware Availability: Apr-2007 Tested by: Sun Microsystems Software Availability: Jul-2007

Operating System Notes (Continued)

 The "webconsole" service was turned off using
     svcadm disable webconsole

Platform Notes

Disk notes: The SPEC CPU tests use a 400 GB partition
created from 3x Sun StorageTek 6140 stripe sets.  The
partition was created in 3 steps: 1. Each 6140 stripe
set (RAID 0) is based on 8x 146 GB 15,000 RPM Seagate
ST3146954FC FC-AL disks.  2. Solaris views these as 3
logical units (LUNs) which are striped together (RAID
0) to make a 3 TB volume using Solaris Volume Manager
(SVM).  3. Lastly, SVM is then used to create one 400
GB soft partition for use by the CPU2006 output_root.

"CMU" = CPU/Memory Unit; each holds 2 or 4 CPU chips.

Memory is 8-way interleaved by filling all slots with
the same capacity DIMMs.

This result was measured using a Sun SPARC Enterprise
M8000 Server.  Note that the Fujitsu SPARC Enterprise
M8000 and Sun SPARC Enterprise M8000 are electrically
equivalent.

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Base Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC 403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M8000

SPECint_rate2006 = 335

SPECint_rate_base2006 = 285

CPU2006 license: 6 Test date: Mar-2007 Test sponsor: Sun Microsystems Hardware Availability: Apr-2007 Tested by: Sun Microsystems Software Availability: Jul-2007

Base Optimization Flags

C benchmarks:

-fast -fma=fused -xcache=128/64/2:5120/256/10 -xipo=2 -xpagesize=4M
-xprefetch_level=2 -lbsdmalloc

C++ benchmarks:

-xdepend -library=stlport4 -fast -fma=fused
-xcache=128/64/2:5120/256/10 -xipo=2 -xpagesize=4M -xprefetch_level=2
-lbsdmalloc

Base Other Flags

C benchmarks:

-xjobs=16 -V -#

C++ benchmarks:

-xjobs=16 -verbose=diags,version

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Peak Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Peak Optimization Flags

C benchmarks:

400.perlbench: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M
-xalias_level=std -Xc -xipo=2 -xrestrict -fma=fused
-xprefetch=latx:5 -lfast

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M8000

SPECint_rate2006 = 335

SPECint_rate_base2006 = 285

CPU2006 license: 6 Test date: Mar-2007 Test sponsor: Sun Microsystems Hardware Availability: Apr-2007 Tested by: Sun Microsystems Software Availability: Jul-2007

Peak Optimization Flags (Continued)

401.bzip2: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M
-xalias_level=strong -fma=fused -xprefetch=latx:5

403.gcc: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M -xipo=2
-xalias_level=std -xprefetch_level=2 -xarch=v8plusb
-fma=fused -ll2amm

429.mcf: -fast -xcache=128/64/2:5120/256/10 -xpagesize=4M -xipo=2

-xprefetch_level=2 -xrestrict -xalias_level=std
-W2,-Apf:llist=3 -W2,-Apf:noinnerllist -xprefetch=latx:5
-lfast

445.gobmk: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M
-xalias_level=std -xrestrict -fma=fused

456.hmmer: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M -xipo=2
-fma=fused

458.sjeng: Same as 456.hmmer

462.libquantum: -fast -xcache=128/64/2:5120/256/10 -xpagesize=4M -xipo=2

-xprefetch_level=2 -fma=fused -xprefetch=latx:3
-lbsdmalloc

464.h264ref: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M -xipo=2
-xalias_level=std -xarch=v8plusb -ll2amm

C++ benchmarks:

471.omnetpp: -xdepend -library=stlport4

-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M
-xalias_level=compatible -xipo=2 -xprefetch_level=2
-Qoption cg -Qlp-av=0 -fma=fused -lfast

473.astar: -xdepend -library=stlport4 -fast

-xcache=128/64/2:5120/256/10 -xpagesize=4M
-xalias_level=compatible -xipo=2 -xprefetch_level=2
-fma=fused -xprefetch=latx:5 -lfast

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 6 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M8000

SPECint_rate2006 = 335

SPECint_rate_base2006 = 285

CPU2006 license: 6 Test date: Mar-2007 Test sponsor: Sun Microsystems Hardware Availability: Apr-2007 Tested by: Sun Microsystems Software Availability: Jul-2007

Peak Optimization Flags (Continued)

483.xalancbmk: -xdepend -library=stlport4

-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -fast
-xcache=128/64/2:5120/256/10 -xpagesize=4M
-xalias_level=compatible -xipo=2 -xprefetch_level=2
-fma=fused -xprefetch=latx:5 -lfast

Peak Other Flags

C benchmarks:

-xjobs=16 -V -#

C++ benchmarks:

-xjobs=16 -verbose=diags,version

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12.20090714.02.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12.20090714.02.xml

Originally published on 1 May 2007.

Report generated on Tue Jul 22 11:33:24 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance